RJFlash.zip:
RJFlash.exe: RJ Uploader Firmware
CDM211226_Setup .exe: FDTI drivers necessary for the USB communication
 
MERLIN_1.XX.s : Firmware Merlin.

All files must be installed in the same folder.
To do the upload a USB/Mini-A USB cable (3m maximum in one length) is needed.
 
The Merlin followspot must not be powered. 
 
•	Remove the Torx screw from the small plate held also by a rivet. It is located on the bottom left of the ballast module on the display side.
•	Slide the plate to have access to the Mini-A USB socket.
•	Connect the USB cable
•	Run first CDM211226_Setup .exe to install the FDTI drivers
•	Run RJFlash.exe. A DOS window should appear
•	Press 1 and Press Enter
•	Select the Firmware number as required and Press Enter
•	The upload shall start and the progression will be shown in percentage. It can take up to 5 minutes to finish.
•	After completion Quit and remove the USB cable

--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------

Merlin RJFlash.zip:
RJFlash.exe: Programme pour mettre à jour les produits RJ
CDM v2.12.00 WHQL Certified.exe: drivers FDTI nécessaires à la communication USB
 
MERLIN_1XX.s : Firmware Merlin.


Tout les fichiers doivent être installés dans le même dossier.
Un cable USB/Mini-A USB est nécessaire pour la mise à jour (3m maximum en une seule longueur).
 
La poursuite Merlin ne doit pas être alimentée. 
 
•	Enlever la vis à empreinte Torx de la petite platine recouvrant le connecteur Mini-A USB qui est aussi maintenue par un rivet. Elle se trouve en bas à gauche du tiroir ballast du coté de l'afficheur.
•	Faire pivoter la petite plaque afin de faire apparaitre le connecteur Mini-A/USB.
•	Connecter le cable USB.
•	Installer les drivers FTDI avec CDM211226_Setup .exe.
•	Lancer RJFlash.exe, une fenêtre Windows DOS doit appaître.
•	Presser sur 1 puis sur Enter.
•	Selectionner le numéro du fichier de mise à jour désiré puis presser sur Enter.
•	La mise à jour démarre et la progression s'affiche en pourcentage. La durée peut prendre jusqu'à 5 minutes.
•	A la fin du processus presser Quit et enlever le cable USB.

